With its broad range of options and configurations, Universal Patch fittings are ideal for almost any design. Tempered glass assemblies are provided with fixed parts in a variety of arrangements - with corner fittings or fin fittings at different angles, and with double or single-action doors in single-leaf or double-leaf designs. Universal fittings are supplied standard with gaskets to suit 10mm and 12mm glass.